

**How to Program the SureBatch Remote**

This Remote is programed from Surefire Ag Systems to work with this specific controller. In the event that the remote fails to operate follow these instructions…

**Step 1:** Locate the create button on the back of remote.



**Step 2:** Insert paper clip into hole and push button until blue light flashes




**Step 3:** While blue light is flashing turn remote over then starting from bottom left push the numbers in numerical order 1 through 8. Number 1 on this remote is the start, button 2 is stop, 3 is above the start button, 4 is above stop, 5 is R3, 6 is R4, 7 is R1 and 8 is R2. Buttons 1-8 must be pushed in numerical order while the blue light flashes. This will create a code for the remote.

(Note buttons 1 & 3 are hidden by sticker see picture below)




**Step 4:** Learning the remote. Power up the SureBatch Controller. Select the run tab.

**Step 5:** Select the setup tab.



**Step 6:** Select the Maint. Tab



**Step 7**: Select the learn remote tab and a blue light under the power button will flash, while flashing hold down the start button until the green light turns on.



Your remote should now be synced with the controller.